**How to update the SBC file in HughesNet HT2000W Systems:**

1. Once the modem is connected to your computer via a wired or wireless connection and powered up, open your browser *(Chrome, Firefox, Internet Explorer, Safari, etc.)* and enter <http://192.168.0.1> in the address bar and click enter!  Do not enter it into a SEARCH box or it WILL NOT work, you MUST enter that address in the address bar of your browser window.
2. At the top of the page to the right of the Language Selection Drop-down box, click on the somewhat hidden “i” icon to the right of the Language selection box on top of that page to get to the “Advanced” page in the modem.
3. Next, in the left column menu, select “Installation” and then “Advanced” and then “Upload SBC Config”
4. **Browse to where you saved the extracted files from the downloaded SBC file and select the .bin file and continue!**
5. You should get a  little confirmation box that pops up and confirms a successful installation! If you get green check marks, you should be good to go!

You can now go back to the System Status page at <http://192.168.0.1>